****

**Technical Bulletin – June 11, 2015**

**360 Y-DROP™ Variable Rate Nozzles**

It has come to our attention that the charts for variable rate nozzles in the 360 Y-DROP Technical Guide, provided by Greenleaf, have some errors that are giving incorrect application rates based on pressure. A new accurate chart is below.

In many cases, there will be no issue reaching the desired application rate. Issues may occur in 22 in. and 20 in. rows, and in 30 in. rows where 02 nozzles are being used with application rates below 15 GPA. In these cases, the 02 nozzles should be replaced with 015 nozzles.

For example:

* 015 nozzles will get 10-24 GPA at 8-9 mph
* 02 will get 15-34 GPA at 8-9 mph

If you have customers and 360 Y-DROP systems affected, please reach out to your Regional Agronomy Manger or contact the Support Center at 888-512-4890 and we will expedite shipping of 015 nozzles to you.